1999 Fletcher Waterman Hills Map
GIS File Description

This file identifies what information can be found in each GIS file.

mwcleav.e00: Point coverage containing cleaveage data.
mwconts.e00: Arc coverage containing contact data.
mwfldsym.e00: Point coverage containing fold symbol data.
mwfolds.e00: Arc coverage containing fold data.
mwfoliat.e00: Point coverage containing foliation data.
mwjoints.e00: Point coverage containing joint data.
mwlabels.e00: Point coverage containing rock unit labels.
mwlineat.e00: Point coverage containing lineation data.
mwnfault.e00: Point coverage containing bar and ball data for normal faults.
mwrocks.e00: Polygon coverage containing rock unit data.
mwstrdip.e00: Point coverage containing strike and dip data.
scalebar.e00: Polygon coverage containing the scalebar.
tbarstw.e00: Arc coverage. Topographic map for Mitchel Range and Waterman Hills, Barstow quad.
tnebo1.e00: Arc coverage. Topographic map for Mitchel Range and Waterman Hills, Nebo quad
tnebo2.e00: Arc coverage. Topographic map for Mitchel Range and Waterman Hills, Nebo quad
